参考文献

[1] 韦东山. 嵌入式Linux应用开发完全手册[M]. 人民邮电出版社，2008

[2] JONATHAN CORBET,ALESSANDRO RUBINI & GREG KROAH-HARTMAN，

Linux设备驱动程序[M] 中国电力出版社 2006

[3] Michael Kerrisk. Linux/UNIX系统编程手册[M](上/下册). 人民邮电出版社，2014

[4] Robert Love. Linux内核设计与实现[M]. 人民邮电出版社 2011.6

[5] Light and Versatile Graphics Library, "Quick overview,"

lvgl.io LVGL LLC. Apr 17, 2021.[Online]. Available:

<https://docs.lvgl.io/v7/en/html/get-started/quick-overview.html>

[6] Light and Versatile Graphics Library, "Porting,"

lvgl.io LVGL LLC. Apr 17, 2021.[Online]. Available:

https://docs.lvgl.io/v7/en/html/porting/index.html

[7] Allwiner Technology, "F1C100s Datasheet,"

F1C600 datasheet, Nov. 2015[Revised Nov.10 2015]

[8] Allwiner Technology, "F1C600 User Manual,"

F1C600 datasheet, Nov. 2015[Revised Nov.10 2015]

[9] SanDisk Corporation, "iNAND Standard and Ultra

e.MMC 4.41 I/F," SDIN5D2-4G-LT datasheet, Mar. 2011[Revised Dec. 2011]

[10] IEEE, "How to Cite References:

IEEE Documentation Style," IEEE Citation Guidelines,

ieee-dataport.org. Available:

<https://ieeedataport.org/sites/default/files/analysis/27/IEEE%20Citation%20Guidelines.pdf>

[11] TORIEX, “Low ESR Cap. Compatible Positive Voltage Regulators”, XC6206 Series datasheet,[2013]

[12] PowTech, “White LED Step-Up Converter”, PT4103 datasheet, [Revised 2017]

[13] EVER ANALOG, “3CH Power Management IC”, EA3036 datasheet, [Revised ]

[14] ShenZhen Nsiway Technology Co, “4-Wire Touch Screen Controller with I2C Interface”, NS2009 datasheet, [2011. 08]

[15] Winbond, “SPI Flash 3V 128M-BIT SERIAL FLASH MEMORY WITH DUAL/QUAD SPI”, W25Q128JV datasheet, [Revised 2016]

[16] NXP, “NTAG I2C – Energy harvesting NFC forum Type 2 Tag with field detection pin and I2C interface”, NT3H1201 datasheet[Revised 2017]

[17] 乐鑫科技, “高性能无线SoC”, ESP8089 datasheet[2016.08]